* [R1] If (SENSOR\_CAHAYA is GELAP) and (SENSOR\_AIR is BASAH) then (MOTOR is TUTUP) (1)
* [R2] If (SENSOR\_CAHAYA is GELAP) and (SENSOR\_AIR is LEMBAB) then (MOTOR is TUTUP) (1)
* [R3] If (SENSOR\_CAHAYA is GELAP) and (SENSOR\_AIR is KERING) then (MOTOR is TUTUP) (1)
* [R4] If (SENSOR\_CAHAYA is MENDUNG) and (SENSOR\_AIR is BASAH) then (MOTOR is BUKA) (1)
* [R5] If (SENSOR\_CAHAYA is MENDUNG) and (SENSOR\_AIR is LEMBAB) then (MOTOR is BUKA) (1)
* [R6] If (SENSOR\_CAHAYA is MENDUNG) and (SENSOR\_AIR is KERING) then (MOTOR is TUTUP) (1)
* [R7] If (SENSOR\_CAHAYA is TERIK) and (SENSOR\_AIR is BASAH) then (MOTOR is BUKA) (1)
* [R8] If (SENSOR\_CAHAYA is TERIK) and (SENSOR\_AIR is LEMBAB) then (MOTOR is BUKA) (1)
* [R9] If (SENSOR\_CAHAYA is TERIK) and (SENSOR\_AIR is KERING) then (MOTOR is STOP) (1)